**Gear Inspection Checklist**

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

* No broken or nicked strands on ropes
* No signs of damage in cores of ropes
* All blocks, pulleys, rings, and port-a-wraps clear of burrs or anything that could snag and damage ropes
* Locking mechanisms functional on all carabiners
* All saddles free of defects and damage that could result in failure or personal injury

Name of inspector:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

* No broken or nicked strands on ropes
* No signs of damage in cores of ropes
* All blocks, pulleys, rings, and port-a-wraps clear of burrs or anything that could snag and damage ropes
* Locking mechanisms functional on all carabiners
* All saddles free of defects and damage that could result in failure or personal injury

Name of inspector:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

* No broken or nicked strands on ropes
* No signs of damage in cores of ropes
* All blocks, pulleys, rings, and port-a-wraps clear of burrs or anything that could snag and damage ropes
* Locking mechanisms functional on all carabiners
* All saddles free of defects and damage that could result in failure or personal injury

Name of inspector:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_